Device-Tree bindings for hdmiphy driver

Required properties:
- compatible: value should be "samsung,exynos5-hdmiphy".
- reg: I2C address of the hdmiphy device.

Example:

	hdmiphy {
		compatible = "samsung,exynos5-hdmiphy";
		reg = <0x38>;
	};
