
Required properties:
- compatible: "ti,tca8418"
- reg: the I2C address
- interrupts: IRQ line number, should trigger on falling edge
- keypad,num-rows: The number of rows
- keypad,num-columns: The number of columns
- linux,keymap: Keys definitions, see keypad-matrix.
