Device-Tree bindings for hdmiddc driver

Required properties:
- compatible: value should be "samsung,exynos5-hdmiddc".
- reg: I2C address of the hdmiddc device.

Example:

	hdmiddc {
		compatible = "samsung,exynos5-hdmiddc";
		reg = <0x50>;
	};
