* Freescale i.MX non-core registers

Required properties:
- #index-cells: Cells used to descibe usb controller index. Should be <1>
- compatible: Should be one of below:
	"fsl,imx6q-usbmisc" for imx6q
- reg: Should contain registers location and length

Examples:
usbmisc@02184800 {
	#index-cells = <1>;
	compatible = "fsl,imx6q-usbmisc";
	reg = <0x02184800 0x200>;
};
