USB PHY

OMAP USB2 PHY

Required properties:
 - compatible: Should be "ti,omap-usb2"
 - reg : Address and length of the register set for the device. Also
add the address of control module dev conf register until a driver for
control module is added

This is usually a subnode of ocp2scp to which it is connected.

usb2phy@4a0ad080 {
	compatible = "ti,omap-usb2";
	reg = <0x4a0ad080 0x58>,
	      <0x4a002300 0x4>;
};
