NVIDIA Tegra audio complex

Required properties:
- compatible : "nvidia,tegra-audio-wm8903"
- nvidia,model : The user-visible name of this sound complex.
- nvidia,audio-routing : A list of the connections between audio components.
  Each entry is a pair of strings, the first being the connection's sink,
  the second being the connection's source. Valid names for sources and
  sinks are the WM8903's pins, and the jacks on the board:

  WM8903 pins:

  * IN1L
  * IN1R
  * IN2L
  * IN2R
  * IN3L
  * IN3R
  * DMICDAT
  * HPOUTL
  * HPOUTR
  * LINEOUTL
  * LINEOUTR
  * LOP
  * LON
  * ROP
  * RON
  * MICBIAS

  Board connectors:

  * Headphone Jack
  * Int Spk
  * Mic Jack

- nvidia,i2s-controller : The phandle of the Tegra I2S1 controller
- nvidia,audio-codec : The phandle of the WM8903 audio codec

Optional properties:
- nvidia,spkr-en-gpios : The GPIO that enables the speakers
- nvidia,hp-mute-gpios : The GPIO that mutes the headphones
- nvidia,hp-det-gpios : The GPIO that detect headphones are plugged in
- nvidia,int-mic-en-gpios : The GPIO that enables the internal microphone
- nvidia,ext-mic-en-gpios : The GPIO that enables the external microphone

Example:

sound {
	compatible = "nvidia,tegra-audio-wm8903-harmony",
		     "nvidia,tegra-audio-wm8903"
	nvidia,model = "tegra-wm8903-harmony";

	nvidia,audio-routing =
		"Headphone Jack", "HPOUTR",
		"Headphone Jack", "HPOUTL",
		"Int Spk", "ROP",
		"Int Spk", "RON",
		"Int Spk", "LOP",
		"Int Spk", "LON",
		"Mic Jack", "MICBIAS",
		"IN1L", "Mic Jack";

	nvidia,i2s-controller = <&i2s1>;
	nvidia,audio-codec = <&wm8903>;

	nvidia,spkr-en-gpios = <&codec 2 0>;
	nvidia,hp-det-gpios = <&gpio 178 0>; /* gpio PW2 */
	nvidia,int-mic-en-gpios = <&gpio 184 0>; /*gpio PX0 */
	nvidia,ext-mic-en-gpios = <&gpio 185 0>; /* gpio PX1 */
};

