* Marvell sdhci-dove controller

This file documents differences between the core properties in mmc.txt
and the properties used by the sdhci-pxav2 and sdhci-pxav3 drivers.

- compatible: Should be "marvell,dove-sdhci".

Example:

sdio0: sdio@92000 {
	compatible = "marvell,dove-sdhci";
	reg = <0x92000 0x100>;
	interrupts = <35>;
};
