* ARASAN PATA COMPACT FLASH CONTROLLER

Required properties:
- compatible: "arasan,cf-spear1340"
- reg: Address range of the CF registers
- interrupt-parent: Should be the phandle for the interrupt controller
  that services interrupts for this device
- interrupt: Should contain the CF interrupt number

Example:

	cf@fc000000 {
		compatible = "arasan,cf-spear1340";
		reg = <0xfc000000 0x1000>;
		interrupt-parent = <&vic1>;
		interrupts = <12>;
	};
