* OMAP OCP2SCP - ocp interface to scp interface

properties:
- compatible : Should be "ti,omap-ocp2scp"
- #address-cells, #size-cells : Must be present if the device has sub-nodes
- ranges : the child address space are mapped 1:1 onto the parent address space
- ti,hwmods : must be "ocp2scp_usb_phy"

Sub-nodes:
All the devices connected to ocp2scp are described using sub-node to ocp2scp
