NXP LPC32xx SoC NAND MLC controller

Required properties:
- compatible: "nxp,lpc3220-mlc"
- reg: Address and size of the controller
- interrupts: The NAND interrupt specification
- gpios: GPIO specification for NAND write protect

The following required properties are very controller specific. See the LPC32xx
User Manual 7.5.14 MLC NAND Timing Register (the values here are specified in
Hz, to make them independent of actual clock speed and to provide for good
accuracy:)
- nxp,tcea_delay: TCEA_DELAY
- nxp,busy_delay: BUSY_DELAY
- nxp,nand_ta: NAND_TA
- nxp,rd_high: RD_HIGH
- nxp,rd_low: RD_LOW
- nxp,wr_high: WR_HIGH
- nxp,wr_low: WR_LOW

Optional subnodes:
- Partitions, see Documentation/devicetree/bindings/mtd/partition.txt

Example:

	mlc: flash@200A8000 {
		compatible = "nxp,lpc3220-mlc";
		reg = <0x200A8000 0x11000>;
		interrupts = <11 0>;
		#address-cells = <1>;
		#size-cells = <1>;

		nxp,tcea-delay = <333333333>;
		nxp,busy-delay = <10000000>;
		nxp,nand-ta = <18181818>;
		nxp,rd-high = <31250000>;
		nxp,rd-low = <45454545>;
		nxp,wr-high = <40000000>;
		nxp,wr-low = <83333333>;
		gpios = <&gpio 5 19 1>; /* GPO_P3 19, active low */

		mtd0@00000000 {
			label = "boot";
			reg = <0x00000000 0x00064000>;
			read-only;
		};

		...

	};
