Texas Instruments DaVinci Platforms Device Tree Bindings
--------------------------------------------------------

DA850/OMAP-L138/AM18x Evaluation Module (EVM) board
Required root node properties:
    - compatible = "ti,da850-evm", "ti,da850";

EnBW AM1808 based CMC board
Required root node properties:
    - compatible = "enbw,cmc", "ti,da850;

Generic DaVinci Boards
----------------------

DA850/OMAP-L138/AM18x generic board
Required root node properties:
    - compatible = "ti,da850";
