Chinese translated version of Documentation/arm64/memory.txt

If you have any comment or update to the content, please contact the
original document maintainer directly.  However, if you have a problem
communicating in English you can also ask the Chinese maintainer for
help.  Contact the Chinese maintainer if this translation is outdated
or if there is a problem with the translation.

Maintainer: Catalin Marinas <catalin.marinas@arm.com>
Chinese maintainer: Fu Wei <tekkamanninja@gmail.com>
---------------------------------------------------------------------
Documentation/arm64/memory.txt 的中文翻译

如果想评论或更新本文的内容，请直接联系原文档的维护者。如果你使用英文
交流有困难的话，也可以向中文版维护者求助。如果本翻译更新不及时或者翻
译存在问题，请联系中文版维护者。

英文版维护者： Catalin Marinas <catalin.marinas@arm.com>
中文版维护者： 傅炜  Fu Wei <tekkamanninja@gmail.com>
中文版翻译者： 傅炜  Fu Wei <tekkamanninja@gmail.com>
中文版校译者： 傅炜  Fu Wei <tekkamanninja@gmail.com>

以下为正文
---------------------------------------------------------------------
		     Linux 在 AArch64 中的内存布局
		     ===========================

作者: Catalin Marinas <catalin.marinas@arm.com>
日期: 2012 年 02 月 20 日

本文档描述 AArch64 Linux 内核所使用的虚拟内存布局。此构架可以实现
页大小为 4KB 的 4 级转换表和页大小为 64KB 的 3 级转换表。

AArch64 Linux 使用页大小为 4KB 的 3 级转换表配置，对于用户和内核
都有 39-bit (512GB) 的虚拟地址空间。对于页大小为 64KB的配置，仅
使用 2 级转换表，但内存布局相同。

用户地址空间的 63:39 位为 0，而内核地址空间的相应位为 1。TTBRx 的
选择由虚拟地址的 63 位给出。swapper_pg_dir 仅包含内核（全局）映射，
而用户 pgd 仅包含用户（非全局）映射。swapper_pgd_dir 地址被写入
TTBR1 中，且从不写入 TTBR0。


AArch64 Linux 内存布局：

起始地址			结束地址			大小		用途
-----------------------------------------------------------------------
0000000000000000	0000007fffffffff	 512GB		用户空间

ffffff8000000000	ffffffbbfffeffff	~240GB		vmalloc

ffffffbbffff0000	ffffffbbffffffff	  64KB		[防护页]

ffffffbc00000000	ffffffbdffffffff	   8GB		vmemmap

ffffffbe00000000	ffffffbffbbfffff	  ~8GB		[防护页，未来用于 vmmemap]

ffffffbffbe00000	ffffffbffbe0ffff	  64KB		PCI I/O 空间

ffffffbbffff0000	ffffffbcffffffff	  ~2MB		[防护页]

ffffffbffc000000	ffffffbfffffffff	  64MB		模块

ffffffc000000000	ffffffffffffffff	 256GB		内核逻辑内存映射


4KB 页大小的转换表查找：

+--------+--------+--------+--------+--------+--------+--------+--------+
|63    56|55    48|47    40|39    32|31    24|23    16|15     8|7      0|
+--------+--------+--------+--------+--------+--------+--------+--------+
 |                 |         |         |         |         |
 |                 |         |         |         |         v
 |                 |         |         |         |   [11:0]  页内偏移
 |                 |         |         |         +-> [20:12] L3 索引
 |                 |         |         +-----------> [29:21] L2 索引
 |                 |         +---------------------> [38:30] L1 索引
 |                 +-------------------------------> [47:39] L0 索引 (未使用)
 +-------------------------------------------------> [63] TTBR0/1


64KB 页大小的转换表查找：

+--------+--------+--------+--------+--------+--------+--------+--------+
|63    56|55    48|47    40|39    32|31    24|23    16|15     8|7      0|
+--------+--------+--------+--------+--------+--------+--------+--------+
 |                 |    |               |              |
 |                 |    |               |              v
 |                 |    |               |            [15:0]  页内偏移
 |                 |    |               +----------> [28:16] L3 索引
 |                 |    +--------------------------> [41:29] L2 索引 (仅使用 38:29 )
 |                 +-------------------------------> [47:42] L1 索引 (未使用)
 +-------------------------------------------------> [63] TTBR0/1
