* Atmel Watchdog Timers

** at91sam9-wdt

Required properties:
- compatible: must be "atmel,at91sam9260-wdt".
- reg: physical base address of the controller and length of memory mapped
  region.

Example:

	watchdog@fffffd40 {
		compatible = "atmel,at91sam9260-wdt";
		reg = <0xfffffd40 0x10>;
	};
