VIA/Wondermedia VT8500 Timer
-----------------------------------------------------

Required properties:
- compatible : "via,vt8500-timer"
- reg : Should contain 1 register ranges(address and length)
- interrupts : interrupt for the timer

Example:

	timer@d8130100 {
		compatible = "via,vt8500-timer";
		reg = <0xd8130100 0x28>;
		interrupts = <36>;
	};
